Note for radxa_rock_pro_debian_wheezy_141124_nand.img:

* This is the Debian 7.0 server image for Radxa Rock Pro/Lite

* This is an "rockchip update.img format image" for NAND flash, flash it with
  - RKBatchTool (Windows)
  - upgrade_tool uf /path/to/the_nand.img (Linux)
For more information about flashing: http://wiki.radxa.com/Rock/flash_the_image

* After flashing, the first time booting up, it will expand the rootfs to the whole NAND flash.

* SSH is enabled by default, password for user rock is rock, for user root is root.

* Md5sum: 242400014eb9cdf500e36659189bb547  radxa_rock_pro_debian_wheezy_141124_nand.img

* Questions and feedbacks: http://talk.radxa.com/topic/631/radxa-debian-image-release
